<MCC> Integer type. Mobile Country Code (first part of the PLMN code).

<MNC> Integer type. Mobile Network Code (second part of the PLMN code).

<freq> Integer type. Cell frequency.

<PCI> Integer type. Physical cell ID.

<RSRP> Integer type. It indicates the signal of Reference Signal Received Power (see 3GPP

36.214). Range: -140 to -44. Unit: dBm.

<RSRQ> Integer type. It indicates the signal of current Reference Signal Received Quality (see

3GPP 36.214). Range: -20 to -3. Unit: dB.

<srxlev> Integer type. Cell selection RX level value (dB).

<squal> Integer type. Cell selection quality value (dB).

<scs> Integer type. Sub-carrier space.

0 15 kHz

1 30 kHz

2 60 kHz

3 120 kHz

<cellID> String type. Cell identity in hex string.

<TAC> String type. Tracking Area Code in hex string.

<bandwidth> Integer type. Bandwidth.

<band> Integer type. Frequency band.